NOVA SCOTIA POSTING REQUIREMENTS

Nova Scotia’s employment laws require employers to post essential information related to workers' rights, employment standards, health and safety. By having these posters and information readily available, employers fulfil their responsibility to ensure that workers are aware of their rights.

[OCCUPATIONAL HEALTH AND SAFETY ACT](https://www.canlii.org/en/ns/laws/stat/sns-1996-c-7/latest/sns-1996-c-7.html)

All workplaces covered by the Nova Scotia *Occupational Health and Safety Act* (the “OHS Act”)must post the following in a prominent place at the workplace:

* Names and contact information of the health and safety committee members, if applicable.
* Name and contact information of the current health and safety representative, if applicable.
* The minutes of the most recent committee meeting until they are replaced by the minutes of the next committee meeting.
* A current copy of the OHS Act.
* Any code of practice required by the OHS Act or regulations.
* A current phone number for reporting occupational health and safety concerns to the Division (“Division” means the Occupational Health and Safety Division of the Department of Labour and Advanced Education).
* Where five or more employees are regularly employed by the employer, an occupational health and safety policy.
* Any order, compliance notice, notice of appeal or decision and an edited order
* Any application for an appeal and notice of appeal
* An application for a deviation from the regulations
* A copy of the decision on such application

WORKPLACE HEALTH AND SAFETY REGULATIONS

All workplaces covered by the Nova Scotia *Workplace Health and Safety Regulations* must post the following in a prominent place at the workplace:

* The location(s) of all the first aid supplies in the workplace and the name and location or phone number of the first aid attendant, if applicable
* Emergency telephone numbers (in the first aid room)

ADDITIONAL OCCUPATIONAL HEALTH AND SAFETY POSTING REQUIREMENTS

* The names of any gases stored in the workplace and signs prohibiting smoking in any storage area for portable compressed gas cylinders
* A readable statement of a hoisting devices rated load so the operator is able to see it when using the hoist
* The maximum number of revolutions per minute of an abrasive wheel and a grinder on

the wheel and grinder.

* A sign on the outside of a room where electrical components are rated at more than 750 v

phase to phase, that legibly states "Danger - High Voltage"

* The current, valid certification at the entrance of a confined space for however long the confined space is occupied.