## FIRST AID INSPECTION CHECKLIST

First Aid Checklist

(WSIB Regulation 1101 Requirements)

| # of Workers on Site | General Contractor  Responsibilities | First Aid Kit Requirements | 🗷 or 🗹 |
| --- | --- | --- | --- |
| 15 - 199 | Provide and maintain a first aid station with a first aid box, 1 stretcher and 2 blankets.  Ensure that the first aid station is at all times in the charge of a worker who,     * Has a valid emergency first aid certificate and * Works in the immediate vicinity of the station. | A current First Aid manual | ❑ |
| 24 safety pins | ❑ |
| 1 basin, preferably stainless steel | ❑ |
| 48 adhesive dressings individually wrapped | ❑ |
| 2 rolls of 1” adhesive tape | ❑ |
| 12 rolls of 1” gauze bandage | ❑ |
| 48 sterile 3" square gauze pads | ❑ |
| 8 rolls of 2" gauze bandage | ❑ |
| 8 rolls of 4" gauze bandage | ❑ |
| 6 sterile surgical pads suitable for pressure dressings | ❑ |
| 12 triangular bandages | ❑ |
| Splints of assorted sizes | ❑ |
| 2 rolls of splint padding | ❑ |